Lawrence Naidu

1

HOMEWORK 3

1. Op-code is CMP, the operands are CX and DX.

2. (b) MOV BX, 1000H

3. MOV BX,[ 1000H]

6. BL and AL Contain 8CH to 7CH. As a result we get 10AH. 0A also shows up.

Also the carry flag

7. BL is greater than AL

**HOMEWORK 3**

**1. Op-code is CMP and the operands are CX and DX.**

**2. (b) MOV BX, 1000H**

**3. MOV BX, [ 1000H]**

**6. BL and AL Contain 8CH to 7CH. So, we get 10AH. 0A also shows up also the carry flag**

**7. BL is greater than AL**